### Device Usage Page (device_usage_statistics.html)

This HTML page displays the device usage statistics that will be sent to Xilinx. The file also contains predefined XML tags used to simplify processing.
Please verify the contents are okay to send to Xilinx!

Software Version and Target Device
Product Version: | ISE:9.1i | Target Family: | aspartan3
OS Platform: | NT | Target Device: | xa3s200
Project ID (random number) | 3832.1 | Target Package: | ftg256
Date Generated | ???????? 4. ????? 03:42:28 2007 | Target Speed: | -4

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
Registers=11

- Flip-Flops=11

Counters=2

- 27-bit up counter=1
- 3-bit up counter=1

Xors=3

- 1-bit xor2=1
- 1-bit xor4=2

Comparators=1

- 27-bit comparator greatequal=1

Multiplexers=1

- 1-bit 7-to-1 multiplexer=1

MiscellaneousStatistics

- AVG_LUT_FAN_IN=2.600000
- AVG_SIG_FANOUT=1.200000
- LUT=15
- MAX_SIG_FANOUT=2
- PK_NUM_4_INPUT_LUTS=15
- PK_NUM_4_INPUT_LUT_RTS=27
- PK_NUM_BONDED_IOBS=5
- PK_NUM_CYINIT=18
- PK_NUM_CYMUX=34
- PK_NUM_EQUIV_GATES=601
- PK_NUM_IOB_FFS=2
- PK_NUM_JTAG_GATES=5
- PK_NUM_LUTLESS_SLICE_FFS=34
- PK_NUM_SLICELS=28
- PK_NUM_SLICES=28
- PK_NUM_SLICE_FFS=39
- PK_NUM_TOTAL_LUTLESS_REGISTERS=34
- PK_NUM_XBZ_GCLKS=1
- PK_NUM_XOR=26
- SINGLE_LOAD_SIG=12
- TWO_LOAD_SIG=3

NetStatistics

- NumNets_Active=69
- NumNets_Gnd=1
- NumNets_Vcc=1
- NumNodesOfType_Active_CLKPIN=23
- NumNodesOfType_Active_CNTRLPIN=23
- NumNodesOfType_Active_DOUBLE=94
- NumNodesOfType_Active_DUMMY=69
- NumNodesOfType_Active_DUMMYESC=2
- NumNodesOfType_Active_GLOBAL=8
- NumNodesOfType_Active_HUNIHEX=4
- NumNodesOfType_Active_INPUT=94
- NumNodesOfType_Active_IOBOUTPUT=2
- NumNodesOfType_Active_OMUX=57
- NumNodesOfType_Active_OUTPUT=63
- NumNodesOfType_Active_PREBXBY=8
- NumNodesOfType_Active_VFULLHEX=6
- NumNodesOfType_Active_VUNIHEX=4
- NumNodesOfType_Vcc_CNTRLPIN=1
- NumNodesOfType_Vcc_INPUT=2
- NumNodesOfType_Vcc_PREBXBY=2
- NumNodesOfType_Vcc_VCCOUT=3

SiteSummary

- BUFGMUX=1
- BUFGMUX_GCLKMUX=1
- BUFGMUX_GCLK_BUFFER=1
- IOB=5
- IOB_INBUF=2
- IOB_OFF1=2
- IOB_OUTBUF=3
- IOB_PAD=5
- SLICEL=28
- SLICEL_C1VDD=1
- SLICEL_C2VDD=4
- SLICEL_CYMUXF=17
- SLICEL_CYMUXG=17
- SLICEL_F=20
- SLICEL_FFX=19
- SLICEL_FFY=20
- SLICEL_G=22
- SLICEL_GNDF=16
- SLICEL_GNDG=13
- SLICEL_XORF=13
- SLICEL_XORG=13

Configuration Data
BUFGMUX_GCLKMUX

- DISABLE_ATTR=[LOW:1]

IOB_OFF1

- LATCH_OR_FF=[FF:2]
- OFF1_INIT_ATTR=[INIT0:2]

IOB_PAD

- DRIVEATTRBOX=[12:3]
- IOATTRBOX=[LVCMOS25:5]
- SLEW=[SLOW:3]

SLICEL_FFX

- FFX_INIT_ATTR=[INIT0:19]
- FFX_SR_ATTR=[SRLOW:19]
- LATCH_OR_FF=[FF:19]
- SYNC_ATTR=[SYNC:19]

SLICEL_FFY

- FFY_INIT_ATTR=[INIT0:20]
- FFY_SR_ATTR=[SRLOW:20]
- LATCH_OR_FF=[FF:20]
- SYNC_ATTR=[SYNC:20]

Pin Data
BUFGMUX

- I0=1
- O=1
- S=1

BUFGMUX_GCLKMUX

- I0=1
- OUT=1
- S=1

BUFGMUX_GCLK_BUFFER

- IN=1
- OUT=1

IOB

- I=2
- O1=3
- OCE=2
- OTCLK1=2
- PAD=5

IOB_INBUF

- IN=2
- OUT=2

IOB_OFF1

- CE=2
- CK=2
- D=2
- Q=2

IOB_OUTBUF

- IN=3
- OUT=3

IOB_PAD

- PAD=5

SLICEL

- BX=6
- BY=5
- CIN=16
- CLK=21
- COUT=17
- F1=20
- F2=5
- F3=4
- G1=22
- G2=8
- G3=4
- G4=3
- SR=21
- X=2
- XQ=19
- Y=3
- YQ=20

SLICEL_C1VDD

- 1=1

SLICEL_C2VDD

- 1=4

SLICEL_CYMUXF

- 0=17
- 1=17
- OUT=17
- S0=17

SLICEL_CYMUXG

- 0=17
- 1=17
- OUT=17
- S0=17

SLICEL_F

- A1=20
- A2=5
- A3=4
- D=20

SLICEL_FFX

- CK=19
- D=19
- Q=19
- SR=19

SLICEL_FFY

- CK=20
- D=20
- Q=20
- SR=20

SLICEL_G

- A1=22
- A2=8
- A3=4
- A4=3
- D=22

SLICEL_GNDF

- 0=16

SLICEL_GNDG

- 0=13

SLICEL_XORF

- 0=13
- 1=13
- O=13

SLICEL_XORG

- 0=13
- 1=13
- O=13

Tool Usage
Command Line History

- xst -ise <ise_file> -intstyle ise -ifn <fname>.xst -ofn <fname>.syr
- ngdbuild -ise <ise_file> <fname>.ngd
- map -ise <ise_file> -intstyle ise -p xa3s200-ftg256-4 -cm area -pr b -k 4 -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -ise <ise_file> -w -intstyle ise -ol std -t 1 <fname>.ncd <fname>.ncd <fname>.pcf
- trce -ise <ise_file> -intstyle ise -e 3 -s 4 -xml <design> <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf
- bitgen -ise <ise_file> -intstyle ise -f <fname>.ut <fname>.ncd