Connections:
************
g1 , g2 = generation polynomials in binary
f1 , f2 = feedback of the PN codes
k=no of flip-flops _ order of the PN code


Operation:
**********
s = the flip-flops (the shift register)
x = the period of the generation = 2^k – 1
T = How many times the Generator will work
t1 , t2 = temp o/p – used to get the i/p of the XOR
n1,n2 = counters  for t1,t2
o1,o2 = the o/p of  feedback XOR
xo1,xo2 = the o/p of  the o/p XOR
I,Q = o/p of the PN code generator


Interface with serial port:
***************************
prt = the serial port object
Ir = the Parameter(I)  o/p from the Kit _ the i/p from the port
Qr = the Parameter(Q)  o/p from the Kit _ the i/p from the port


Comparing the results:
**********************
testI = user to save the error pattern of I
testQ = user to save the error pattern of Q
INOE = no of errors in I
QNOE = no of errors in Q
ILOE = Location of Wrong bits in I	
QLOE = Location of Wrong bits in Q	
IL , QL = counters for ILOE , QLOE
	
	

